Tobias ====== Feuchte mit großem weissen ====== Device Address: 6703000084DA6E26 (26 6E DA 84 00 00 03 67) Name: DS2438 Alternate Names: Smart Battery Monitor Description: 1-Wire device that integrates the total current charging or discharging through a battery and stores it in a register. It also returns the temperature (accurate to 2 degrees celcius), as well as the instantaneous current and voltage and also provides 40 bytes of EEPROM storage. ====== Doppel switch mit 2 grossen Klemmen und aufgelötetenTEmp ====== ===== Temp ===== Device Address: 0E000009006AA228 (28 A2 6A 00 09 00 00 0E) Name: DS18B20 Alternate Names: DS1820B, DS18B20X Description: Digital thermometer measures temperatures from -55C to 125C in 0.75 seconds (max). +/- 0.5C accuracy between -10C and 85C. Thermometer resolution is programmable at 9, 10, 11, and 12 bits. ===== switch ===== Device Address: A6000000CBC4A512 (12 A5 C4 CB 00 00 00 A6) Name: DS2406 Alternate Names: Dual Addressable Switch, DS2407 Description: 1-Wire Dual Addressable Switch. PIO pin channel A sink capability of typical 50mA at 0.4V with soft turn-on; optional channel B typical 10 mA at 0.4V. 1024 bits of Electrically Programmable Read Only Memory (EPROM) partitioned into four 256 bit pages. 7 bytes of user-programmable status memory to control the device.