Tobias [[https://tm3d.de/]] [[https://tm3d.de/shop]] ====== Feuchte mit großem weissen ====== Device Address: 6703000084DA6E26 (26 6E DA 84 00 00 03 67) Name: DS2438 Alternate Names: Smart Battery Monitor Description: 1-Wire device that integrates the total current charging or discharging through a battery and stores it in a register. It also returns the temperature (accurate to 2 degrees celcius), as well as the instantaneous current and voltage and also provides 40 bytes of EEPROM storage. ====== Doppel switch mit 2 grossen Klemmen und aufgelötetenTEmp ====== ===== Temp ===== Device Address: 0E000009006AA228 (28 A2 6A 00 09 00 00 0E) Name: DS18B20 Alternate Names: DS1820B, DS18B20X Description: Digital thermometer measures temperatures from -55C to 125C in 0.75 seconds (max). +/- 0.5C accuracy between -10C and 85C. Thermometer resolution is programmable at 9, 10, 11, and 12 bits. ===== switch ===== Device Address: A6000000CBC4A512 (12 A5 C4 CB 00 00 00 A6) Name: DS2406 Alternate Names: Dual Addressable Switch, DS2407 Description: 1-Wire Dual Addressable Switch. PIO pin channel A sink capability of typical 50mA at 0.4V with soft turn-on; optional channel B typical 10 mA at 0.4V. 1024 bits of Electrically Programmable Read Only Memory (EPROM) partitioned into four 256 bit pages. 7 bytes of user-programmable status memory to control the device. ==== Bestellungen: ==== Am 01.05.2017 um 15:29 schrieb shop@tm3d.de: Anz. Nr. Beschreibung Preis Gesamt 2 002 Bausatz 1-Wire Feuchte und Temperatur HIH4031 + DS2438 (THT) 20,90€ 41,80€ 1 007 Bausatz 1-Wire Feuchte und Temperatur mit DHT22 und ATTINY84A 11,70€ 11,70€ 1 037 Sensor Gehäuse für die Wand von ITALTRONIC 4,65€ 4,65€ 3 016 Sensor Gehäuse für die Wand 2,30€ 6,90€ 1 017 Kleingehäuse 0,80€ 0,80€ 1 026 1-Wire Barometer/Temperatur/Luftfeuchte 32,80€ 32,80€ 10 030 LSA-Klemme 3,81mm 0,20€ 2,00€ 1 034 Aufsatz für SHT21/SHT25 (Kondensationsschutz) 1,00€ 1,00€ Gesamt Summe: 101,65€